C5GG2DF1 - 206 CABRIOLET

REMOVAL - REFITTING BOOT SIDE TRIM

1 - REMOVAL

Partially remove the boot seal (1) .

On the right-hand side ; Remove :

- the cover with its jack
- the repair kit

Remove :

- the trim mounting clips (2)
- the luggage retaining hook (3)

On the left-hand side ; Remove the boot light .

Remove :

- the fasteners (5)
- the roof support (4)
- the fastener (6)

On the right-hand side ; Remove the support (7) upwards .

On the left-hand side ; Pass the support (7) fitted with its harness through the lights access cut-out .

Detach then remove the trim .

2 - REFITTING

Proceed in the reverse order to removal .