C7AP0QV1 - 206

FITTING FOG LAMP KIT PART NO. 9682.G3

IMPERATIVE : the fog lamp kit part number 9682.G3 must be fitted by a professional .

1 - CONTENTS OF THE FOG LAMP KIT

description | reference | quantity
--- | --- | ---
fog lamp | 1 | 2
bumper cut-out trim | 2 | 2
fog lamp harness | 3 | 1
earth lead (green-yellow) | 4 | 1
LED | 5 | 1
RAYCHEM sleeve | 6 | 2
strip of mastic | 7 | 1
relay | 8 | 1
fuses 10 A | 9 | 2
sleeve (wire feed) | 10 | 1
lighting switch | 11 | 1
securing bolt(s) : fog lamp | 12 | 2
plastic clip 200 mm | 13 | 10
cage nuts | 14 | 2

(A) : Section of the fog lamp harness leading to the fog lamps .

(B) : Section of the fog lamp harness leading to the engine wiring housing .

(C) : Section of the fog lamp harness leading to the passenger compartment .

Remove :

- the battery and detach its plastic unit (according to specification)
- the upper and lower covers and the wiring housing harness

2 - CONNECTION OF THE FOG LAMP HARNESS TO THE ENGINE WIRING HOUSING

Clip :

- the grey wire : to cell J2
- the brown-yellow wire : to cell J1
- the white wire : to cell N1
- the yellow-green wire : to cell N2

The cell markings are engraved under the engine wiring housing .

Fit :

- the fuses 10 A (9) to locations (D)-(E)
- the relay (8) in position (F)

Refit the engine wiring housing .

Remove the rubber closer (G) located to the left of the clutch pedal .

Using a screwdriver, drive out the plastic protective cover from the bottom of the recess to free the bulkhead opening .

3 - ROUTING OF THE FOG LAMP HARNESS

Route the fog lamp harness and clip it along the original harness using plastic clips (13) .

Connect the fog lamp harness yellow-green earth wire to the vehicle earth behind the front left headlight unit .

Engage the harness fitted with the grommet (10) through the vehicle bulkhead in order to determine the position of the grommet on the harness .

4 - SEALING

Seal the grommet (10) on the harness using mastic (7) .

(H) : To the passenger compartment .

5 - CONNECTION OF THE FOG LAMP HARNESS TO THE LIGHTING STALK

Remove :

- the upper and lower steering column cowlings
- the lighting stalk

Disconnect the 2 stalk connectors .

Clip the white wire of the fog lamp harness to the black 10-way connector at way 4B .

Reconnect the 2 connectors to the lighting stalk (11) then refit the stalk .

5 - 1 - FITTING THE FOG LAMP OPERATION WARNING LIGHT

Vehicle fitted with a 3 dial instrument panel .

Drill a 8 mm diameter hole marked at (I) in the steering column upper cowling .

Clip the LED (5) in the hole .

Connection of the fog lamp operation warning light :

- delete the clip from the end of the yellow wire
- strip the end of the yellow wire for 5 mm
- connect the red wire of the LED (5) to the yellow wire of the fog lamp harness using a Raychem sleeve (6)
- connect the black wire of the LED (5) to the yellow-green wire (4) of the fog lamp harness using a Raychem sleeve (6)

Remove :

- partly : the door seal (J) (on the driver's side)
- partly : the carpet (K)

Connect the earth terminal of the yellow-green wire (4) to the vehicle earth (L) .

Clip the yellow-green wire (4) along the original harness using clips (13) .

Refit :

- the carpet
- the door seal
- the steering column finishers

Vehicle fitted with a 4-5 dial instrument panel :

- remove the instrument panel
- open the 26-way connector (yellow)
- insert the clip on the yellow wire into position 3
- close the 26-way connector (yellow)
- resecure the instrument panel

6 - FITTING OF THE FOG LAMPS TO THE BUMPER

Remove :

- grille
- the bumper

Carefully cut the bumper along the inner marking and adjust if necessary .

Fit the cut-out finishing rings (2) marked (G) and (D) .

The marking letter on the trim is to be positioned at the top when fitted to the bumper .

Engage :

- the cage nut (14) in its housing
- the 2 upper plates of the lamp in the bumper locations

Secure the fog lamps (1) to the bumper using bolts (12) .

On the left-hand side : No. 67742320 .

On the right-hand side : No. 67742310 .

Connect the fog lamp harness to the fog lamps .

Fit the bumper .

Place the vehicle on a lift (In order to clip the harness along the front crossmember using clips (13)) .

Return the vehicle to its wheels .

Adjust the fog lamps, vehicle empty .

Refit the mud shields .

(Notice valid subject to product modification) .