B2FH03K1 - 206

REPLACEMENT GAITER BEARING AT GEARBOX END (MB3 DRIVE SHAFT)

1 - SPECIAL TOOLS

reference | description | reference | reference
--- | --- | --- | ---
[1] | stripping device | FACOM U 53 K2 | FACOM U 53 K2

reference | description | reference | reference
--- | --- | --- | ---
[2] | tube for fitting the gaiter bearing at the gearbox end | (-).0410-H | 4608-TG

reference | description | reference | reference
--- | --- | --- | ---
[3] | spider protector | (-).0410-J | (-).0410-J

2 - REPLACEMENT OF THE GAITER BEARING AT THE GEARBOX END

Fit the spider protector .

Mark the position of the spider in relation to the shaft .

Remove :

- the circlip (1)
- the spider (2) using a flat chisel
- the collar (4)
- the drive shaft gaiter (3)

Remove the gaiter bearing .

Fit a new bearing using the tool [2] .

Continue the fitting operations in the reverse order to removal .