B1FD01K1 - 206 DW8 ENGINE TU ENGINE D4D ENGINE MERCOSUR

CHECK OIL PRESSURE

1 - SPECIAL TOOLS

reference | description | reference | reference
--- | --- | --- | ---
[A] | kit for checking pressures and vacuums | (-).1503-ZV | 4103-T
[1] | pressure gauge | (-).1503-AZ | 2279-T
[2] | flexible hose | (-).1503-B | 7001-T
[3] | union | (-).1503-E | 7001-T
[4] | pin | - | 7001-T

2 - PRESSURE CHECK

WARNING : oil pressure is checked with the engine hot after checking the oil level .

Disconnect the oil pressure switch .

Remove the oil pressure switch .

DW8 ENGINE

D4D ENGINE

TU1JP ENGINE EMISSION CONTROL CEE 2000 TU3JP ENGINE EMISSION CONTROL CEE 2000 D4D ENGINE

Remove the oil pressure switch (1) .

D4D ENGINE

Remove the oil pressure switch (1) .

Fit the union [3] .

Connect the pressure gauge [1] and flexible hose [2] .

Connect a tachometer .

read the pressures .

Remove the pressure gauge [1], its hose [2] and its union [3] .

Remove the rev counter .

fit the oil pressure switch using a new washer .

Reconnect the pressure switch .

oil capacity .