E2AK0SK1 - 206

LASHING VEHICLE

1 - TRANSPORTING BY SEA

à minimum: 70° .

Front lashing .

à minimum: 70° .

Rear lashing .

WARNING : the tension of the tie-ropes (1) must not be exerted laterally across the lashing hooks .

2 - TRANSPORTING BY ROAD

Using straps with 3 securing points, placed around the tyres (2 straps minimum) .

At the front of the vehicle :

- using straps and hooks at the front towing eyes

At the rear of the vehicle :

- using straps and hook at the damper upper securing pins, in its direction of operation