C5IG17F1 - 206 CABRIOLET

REMOVAL - REFITTING FRONT MOVING PANEL SIDE SEAL

1 - TOOLING

[1] Tool for positioning the seal nipple (-).1349-B .

[2] Roller (-).1349-G .

2 - REMOVAL

APPLY THE OPERATING PROCEDURE FOR HYDRAULIC PUMP LOAD REDUCTION .

IMMOBILISE THE BOOT COVER .

Lift the roof then place it in the intermediate position for accessibility (Two operators are necessary) .

Unclip the side seal sleeve (1) at (A) .

Unseat the seal (1) .

Unclip the sleeves from the side seal (1) at (B) - (C) .

Pull the seal (1) forwards to unseat it from the flange at (D) .

Remove the moving panel side seal .

3 - REFITTING

Clip the sleeves (B) - (C) in the holes using a tool [1] (Use soapy water to make fitting easier) .

Fit the seal (1) at (D) for a few centimetres .

Position the rear moulding of the seal (1) on the flange (perpendicular to the flange) .

Place the moulding at the stop on the flange .

Clip the sleeve (A) in the hole using the tool [1] .

Fit the seal (1) on the rest of the side flange .

Position the lip (2) on the trim (3) .

Pass the tool [2] over the attachment zone (E) to finish fitting .

Proceed in the reverse order to removal .

Test operation .