B2CB3DK1 - 206 BE4 GEARBOX

IDENTIFICATION OF TIGHTENING TORQUES GEARBOX CONTROLS

1 - IDENTIFICATION

(1) Control rod (Ball joint ø 10) .

(2) Control relay lever (Ball joint ø 10) .

(3) Selection rod .

(4) Engagement rod .

(5) Reaction rod .

(6) Support plate (Ball joint ø 10) .

(7) Selection lever (Ball joint ø 10) .

(8) Engagement lever (Ball joint ø 13) .

2 - TIGHTENING TORQUE(S)

Gear lever to control rod : 0.8 da.Nm .

Relay lever shaft (A) : 3 da.Nm + Loctite .

Support plate fixing (B) to gearbox : 1.5 da.Nm .

Lubricate the shafts and ball joints with ESSO NORVA 275 grease .