B1FD07K1 - 206 EW10J4 ENGINE DW10TD ENGINE

CHECK OIL PRESSURE

1 - SPECIAL TOOLS

EW10J4 ENGINE

[A] Kit for checking pressures and vacuums (-).1503-ZV :

- [1] pressure gauge (-).1503-AZ
- [2] flexible hose (-).1503-B

DW10TD ENGINE

[A] Kit for checking pressures and vacuums (-).1503-ZZ :

- [1] pressure gauge
- [2] flexible hose

[3] union (-).1503-H .

2 - PRESSURE CHECK

WARNING : oil pressure is checked with the engine hot after checking the oil level .

Remove the shield under the power train, (according to specification) .

Place a draining tray under the engine .

DW10TD ENGINE

Remove the oil filter .

EW10J4 ENGINE

Fit tool [3] in place of the oil filter .

Fit the assembly of tools [1] - [2] on tool [3] .

Start the engine .

READ THE PRESSURES .

Remove the tools in the reverse order to fitting .

Fit :

- a new oil filter
- the shield under the power train, (according to specification)

top up the engine oil .