C4BG0QF1 - 206

REMOVAL - REFITTING TAILGATE

1 - REMOVAL

Remove :

- the rear parcel tray
- fold down the rear seat back(s)
- the fasteners (1)
- the quarter light surround (2)

Unclip the electrical connection (3) .

Remove the fastener (4) for the earth lead .

Release the harness (5) .

On the opposite side : Disconnect the screen-washer pipe .

Detach : The grommets (6) for routing the harnesses (5) .

NOTE : for the following operations, two operators are necessary .

Support the tailgate and remove the struts (7) .

Remove :

- the fasteners (8)
- the tailgate

2 - REFITTING

Proceed in the reverse order to removal .

Adjust fits and clearances (If necessary) .