B1FG04K1 - 206 D4D ENGINE MERCOSUR

REMOVAL - REFITTING OIL PUMP

1 - SPECIAL TOOLS

[1] Oil pump positioning tool (-).1355 .

2 - REMOVAL

Drain the engine oil .

Remove :

- stone guard panel
- the accessory belts
- the timing belt
- the oil level sensor
- the dipstick
- the crankshaft pulley
- the crankshaft gear
- the sump

Remove :

- the oil pump strainer (1)
- the oil pump (2)

Clean the joint seals without scratching the aluminium surfaces .

3 - REFITTING

Always replace the oil pressure supply seal (3) .

Place a bead of E10 sealant on the joint seal .

WARNING : the oil pump is driven from the end of the crankshaft by means of two flats .

Fit :

- the oil pump : tightening torque 0.9 da.Nm
- the new seal on the crankshaft output shaft

Replace the strainer fitted with its new o ring .

Clean the seal faces :

- cylinder block
- sump

Fit the sump .

Tighten the bolts to 1 da.Nm .

Fit :

- the timing belt
- the accessory belts

Proceed in the reverse order to removal .