C5KG0BF1 - 206

REMOVAL - REFITTING ELECTRIC SUN ROOF MOVING PANEL

1 - REMOVAL

Open the moving panel by approximately 200 mm .

Remove the drive pins (1) .

Open the moving panel manually as far as possible .

Close the moving panel manually to extract the left and right rails, and the front angle brackets of the moving panel via space (2) .

Two people are required to perform the following operation .

Continue to close the moving panel by 200 mm .

Tilt this moving panel towards the left (3) and continue to close it until the right rear angle bracket and then the left exit via space (2) .

Remove the moving panel .

2 - REFITTING

Check that the pads are in place on the moving panel angle brackets .

Proceed in the reverse order to removal .