C4BG0SF1 - 206 CABRIOLET

REMOVAL - REFITTING LOWER BOOT COVER

1 - REMOVAL

On each side ; Remove the mounting (1) at the top .

Open the luggage compartment .

Disconnect the connectors (A) - (B) - (C) .

Detach the harness from the clips (2) .

Remove the fastener (3) .

Remove the lower side mountings (4) .

Detach then remove the lower boot panel .

2 - REFITTING

Proceed in the reverse order to removal .

ADJUST THE CLEARANCES AND FLUSH FITTING .

Tighten the fasteners (1) - (4) to 0.9 ± 0.1 da.Nm .