C5EH05F1 - 206 CABRIOLET

REMOVAL/REFITTING OF A 3RD BRAKE LIGHT BULB

1 - REMOVAL

Mark the faulty bulb .

REMOVE THE THIRD BRAKE LIGHT .

Remove the support plate fixings (1) .

Remove the support plate (2) from the housing .

Remove then replace the faulty bulb (3) .

2 - REFITTING

Proceed in the reverse order to removal .

IMPERATIVE : check the presence of the seal(s) ; replace the seal(s) if necessary .

Test operation .