C5IM00F1 - 206 CABRIOLET

ROOF OPENING (MANUAL REPAIR PROCEDURE FROM COUPÉ TO CABRIOLET)

Open the luggage compartment .

Unfold the tray (luggage cover screen (1) .

Lower the side windows of the doors and rear quarter panels .

IMMOBILISE THE BOOT COVER .

Using a screwdriver , push in the detachable rear shelf strut as far a possible .

On each side and at the front, release the striker (2) .

NOTE : two people are required to perform the following operation .

Raise the roof at (A) then detach it rearwards .

Manoeuvre the roof to fold it in the boot and place it in contact with the rear stops (B) .

Tilt the moving rear shelf (3) to place it in the exit position .

Remove the hexagonal wrench from the guide .

Fold down the boot cover to the front by lightly pressing in the centre of the cover to counter the residual pressure of the system (C) .

Open the luggage compartment .

On each side :

- pull the u-clip (4) at (D)
- pivot the u-clip (4) and release it at (E)

Check that the boot cover is locked .

Close the boot .

IMPERATIVE : following elimination of the fault, do not forget to return the u-clip (4) to its initial position .