B2CG50K1 - 206 MA GEARBOX

DISMANTLING GEARBOX

Remove the clutch stop (1) .

Place the gearbox on a block of wood (H = 180 mm) (Minimum) .

Remove :

- the mounting and the speedometer take-off gear (2)
- the reverse lamp switch (3)
- gearbox drain plug
- filling and level plug
- the final drive output seals

1st fitting, Remove :

- the ball joint lever (4)
- the clamp (5)
- the connecting plate (6)

2nd fitting :

- remove the gearbox control relay lever (3) (7)