C5HG1AF1 - 206

REMOVAL - REFITTING HEATER BLOWER

1 - REMOVAL

Remove the steering column .

RIGHT HAND DRIVE

Remove the glove box .

ALL MODELS

Pivot the blower anti-clockwise to release it from its housing on the air conditioner (A) .

WARNING : remove the bolt (1) which may be present in some repair fittings .

Pull the blower to release it from the air conditioner .

Pull the blower to release it downwards .

Remove the blower .

Disconnect the connector(s) according to specification .

RIGHT HAND DRIVE

Remove the blower via the storage compartment opening .

ALL MODELS

2 - REFITTING

Proceed in the reverse order to removal .

WARNING : in the event of poor gripping of the blower on refitting, secure the blower using 1 0.4 X 15 mm Torx bolt(s) at (B) on the plate .