C5IG14F1 - 206 CABRIOLET

REMOVAL - REFITTING HYDRAULIC CENTRAL UNIT

1 - REMOVAL

Change the vehicle into the coupé version .

Open the boot .

REMOVE THE UPPER TRIM FROM THE CONTROL UNIT .

CARRY OUT THE LOAD REDUCTION OPERATION FOR THE HYDRAULIC UNIT .

Remove :

- the retaining straps (1)
- the sound-proofing cover (2)

Cut the tie-wraps (A) .

Disconnect the connector (3) .

Remove :

- the hydraulic pipes (4) - (5)
- the hydraulic central unit (6)

2 - REFITTING

mark(s) on the hydraulic pipe(s)
struts | input | outlet
--- | --- | ---
left roof strut | 11 | 12
right roof strut | 13 | 14
moving shelf strut | 17 | 18
boot left strut | - | -
boot right strut | 15 | 16

WARNING : observe strictly the above order and fit new copper seals .

Tighten :

- the fastenings (4) to 1 ± 0.25 da.Nm
- the fastenings (5) to 1.2 ± 0.35 da.Nm

Continue the fitting operations in the reverse order to removal .

Test operation .

CHECK THE FLUID LEVEL .