C5KG0HF1 - 206

REMOVAL - REFITTING ELECTRIC SUN ROOF HEADLINING

1 - REMOVAL

Remove :

- the sun visors
- the sun visor retaining hooks
- the roof console
- partly : the screen pillar trim pads
- the grab handles or blanks
- the seat belt upper mountings
- the central pillar trims
- the roof lamp

Partly release the quarter panel trims, without releasing the seat belt .

Remove : The sun roof frame finishing seal (1) .

Release the headlining from the door seals .

Two people are required to perform the following operation .

Unclip all the pieces of velcro (2) to separate the sun roof frame from the roof .

Allow the headlining to rest on the seats .

Remove the headlining rearwards .

2 - REFITTING

Proceed in the reverse order to removal .

Tightening torque(s) :

- the seat belt attachment : to 3 da.Nm