C4CH1VF1 - 206 CABRIOLET

REPLACEMENT REAR QUARTER PANEL WATER SEALING FILM

1 - REMOVAL

Remove :

- THE REAR QUARTER PANEL FINISHER PANEL
- the mounting on the front seat belt ecu

Disconnect and detach the front seat belt ecu .

REMOVE THE AIR SEALING FILM .

Remove the water sealing film .

2 - REFITTING

Remove dirt from the panel flange (Degrease using dilute surface cleaner) .

IMPERATIVE : always change the sealing sheet after every operation .

Proceed in the reverse order to removal .

IMPERATIVE : fit new seals, which must be assembled without folds and tears ; the bearing surface on the interior panel needs to absolutely clean ; these recommendations are essential to prevent possible entry of water, dust or noise .