C4CG23F1 - 206 CABRIOLET

REMOVAL - REFITTING DOOR TRIM PAD

1 - SPECIAL TOOLS

[1] Trim pliers (-).1311 .

2 - REMOVAL

Open the door .

Lower the glass fully .

REMOVE THE MIRROR CHEATER .

Remove the securing bolts (1) .

Remove the interior opening control trim (2) using a flat screwdriver .

Unclip the panel using the tool [1] .

Detach the panel from the weatherstrip, detaching it upwards .

Remove the door trim pad .

3 - REFITTING

Proceed in the reverse order to removal .