B2BE02K1 - 206 MA GEARBOX

CHECK - ADJUSTMENT CLUTCH CONTROL

1 - PRELIMINARY OPERATIONS

RIGHT HAND DRIVE

LEFT HAND DRIVE

ALL MODELS

Check :

- that there is no obstacle (mat etc.) to the clutch pedal travel
- the fitting of the clutch cable on the bulkhead (A)
- the routing of the clutch cable

RIGHT HAND DRIVE

Check the clamping of the clutch cable to the bulkhead .

ALL MODELS

2 - CHECK - ADJUSTMENT

Check that there is a minimum clearance (X) .

If there is not, adjust the bolt (1) .

NOTE : if the clearance (X) is too great this could result in a creaking sound .

Pull the cable at (B) :

- if the cable moves (minimum 5 mm): the clutch cable is adjusted
- if the cable does not move: replace the clutch cable

Check the travel of the clutch cable .

If Y ≥ 24 mm :

- adjustment correct

If Y : Less than 24 mm :

- replace the clutch cable