C4CG26F1 - 206 CABRIOLET

REMOVAL - REFITTING REAR QUARTER PANEL INTERIOR WEATHERSTRIP SEAL

1 - REMOVAL

Place the vehicle in cabriolet position .

IMMOBILISE THE BOOT COVER .

REMOVE THE REAR QUARTER PANEL WEATHERSTRIP END PIECE .

Remove the clips (1) .

Detach the weatherstrip (2) upwards .

2 - REFITTING

NOTE : apply a product to assist fitting on the flange (example: soapy water) .

Engage the weatherstrip (2) at the rear .

Engage the other end of the seal on the flange, then fit the rest of the seal .

Fit new clips (1) .

Engage the sleeve (3) in the boot lower seal .

Continue the fitting operations in the reverse order to removal .