C4AH1IF1 - 206 CABRIOLET

REPLACEMENT FRONT PILLAR

IMPERATIVE : THIS VEHICLE HAS BEEN DESIGNED USING THE MIG BRAZING PROCESS TECHNIQUE ; when the structure is repaired, all the connections concerned must be welded using the same procedure ; any other technique is prohibited .

WARNING : all the scoured areas must be protected by the approved electrolytic re-zincing process .

IMPERATIVE : observe elementary health and safety rules (wearing of filter mask for organic fumes - work in a ventilated area) .

1 - COMPLEMENTARY OPERATION(S)

Replacement :

- FRONT DOOR
- FRONT WING

Removal - refitting :

- WINDSCREEN
- bonnet hinges
- scuttle grille
- FASCIA
- door aperture seals
- FRONT SEAT
- bonnet

Remove-refit trim :

- part front floor
- front pillar
- WINDSCREEN PILLARS

Detach the electrical harnesses .

2 - IDENTIFICATION OF REPLACEMENT PARTS

Passenger compartment side front stiffener .

Front pillar .

3 - REPLACEMENT PART COMPOSITION

(1) Passenger compartment side front stiffener .

(2) Front pillar .

(3) Front wing fixing bracket .

4 - PART(S) REQUIRED TO CARRY OUT THE OPERATION

Passenger compartment side front stiffener .

Front pillar .

5 - PREPARATION OF THE NEW PART

6 - CUTTING OUT

7 - RELEASING

8 - ADJUSTMENT

9 - WELDING

10 - FINISHING

11 - SEALING

12 - PROTECTION