B2CG80K1 - 206 AL4 AUTOMATIC GEARBOX

REMOVAL - REFITTING HEAT EXCHANGER FLOW CONTROL SOLENOID

1 - REMOVAL

NOTE : do not drain the gearbox .

Disconnect the battery .

Remove :

- the ECU cover
- the connector of the engine ecu
- the battery
- the battery container
- the air cleaner housing
- the air hose

Remove the 2 bolts (1) (Mounting of the modular connector on the gearbox) .

Disconnect the modular connector (2) .

Extract the blue 3-way connector (3) from the modular connector (2) .

Remove :

- the front left-hand wheel
- the solenoid valve harness that controls the exchanger (4) output
- the 2 bolts (5)
- heat exchanger flow control solenoid (4)

2 - REFITTING

Replace the two o rings on the solenoid valve that controls the exchanger (4) output .

Remove :

- heat exchanger flow control solenoid (4)
- the 2 bolts (5) : tightening torque 1 da.Nm
- the solenoid valve harness that controls the exchanger (4) output
- the blue 3-way connector (3) in the modular connector (2)
- the 2 bolts (1) : tightening torque 1 da.Nm

Reconnect the modular connector (2) .

Fit :

- the front left-hand wheel
- the battery container
- the battery
- the air cleaner housing
- the air hose
- the connector of the engine ecu
- the ECU cover

Connect the battery .