C5IG03F1 - 206 CABRIOLET

REMOVAL - REFITTING ELECTRONIC UNIT

1 - REMOVAL

IMPERATIVE : do not switch on the ignition at any time during the operation .

Open the luggage compartment .

REMOVE THE UPPER TRIM FROM THE CONTROL UNIT .

Disconnect the connectors (1) .

Pull the housing (2) towards you to detach it from its support .

Remove the ecu (2) .

2 - REFITTING

Proceed in the reverse order to removal .

Test operation .