B2CI0CV1 - 206

GEARBOX CAPACITY

gearbox - final drive
vehicles | type of gearbox - final drive | number of speeds | capacities in litres
--- | --- | --- | ---
106 | MA BE3 | 4 | -
| MA | 5 | -
| BE1 - BE3 | 4 | -
| BE1 - BE3 | 5 | 2
306 | BE3 | 6 | 2,15
206 - 406 | BE4 | 5 | 1,90
406 - 806 | ML5T | 5 | 1,85
806 | ME5T | 5 | 1,85
imperative : in every case, check the level and top-up if necessary

automatic gearbox
vehicles | type of automatic gearbox | capacities in litres | capacities in litres (after overhaul)
--- | --- | --- | ---
306 | 4HP14 - 4-speed | 2,40 | 6,20
imperative : in every case, check the level and top-up if necessary

electronic automatic gearbox
vehicles | type of electronic automatic gearbox | capacities in litres (after draining and refilling) | capacities in litres (after overhaul)
--- | --- | --- | ---
106 | MB3 - 3-speed | 2,50 | 4,50
406 | 4HP20 - 4-speed | 3,00 | 8,00 ± 0,30
206 - 306 - 406 806 | autoadaptive automatic gearbox 4-speed | 4,50 | 6,00
imperative : in every case, check the level and top-up if necessary