B2CG52K1 - 206 MA GEARBOX

DISMANTLING - ASSEMBLY INPUT SHAFT

1 - SPECIAL TOOLS

reference | description | reference | reference
--- | --- | --- | ---
[1] | universal extractor | FACOM U53T

reference | description | reference | reference
--- | --- | --- | ---
[2] | fitting tool for input shaft spring ring | (-).0317-AK | 8.0313T-M
[3] | tool for fitting input shaft bearings | (-).0317-F | 7.101T-F

2 - PRELIMINARY OPERATIONS

Dismantling : Gearbox .

Removal : Gearbox casing .

Removal : Input, output shafts and differential .

3 - DISMANTLING

Extract the bearing (3) at the 4th speed end .

Extract the bearing (4) at the 1st speed end .

4 - ASSEMBLY

WARNING : bearings removed must not be re-used ; lubricate the components as they are refitted ; check that the shaft bearings are in perfect condition, no knock or scratch marks ; observe the matching, the direction of fitting or the relative positions of re-used parts marked on dismantling ; use parts which are clean and free from faults .

Fit the new bearing (4) on the 1st gear side .

Fit the new bearing (3) on the 4th gear side .

NOTE : position the bearing groove (A) upwards .

5 - COMPLEMENTARY OPERATION(S)

WARNING : observe the cleaning and refitting conditions .

Refitting : Input, output shafts and differential .

Refitting : Gearbox casing .

Assembly : Gearbox .