C4CH1FF1 - 206

REPLACING DOORS (REAR DOOR)

1 - SPECIAL TOOLS

[1] Door stand .

Make 2 blocks [2] in accordance with the diagram .

Make 2 blocks [3] in accordance with the diagram .

Make 2 blocks [4] in accordance with the diagram .

2 - FITTING

Place the door on the stand [1] .

identification of the fixed hinges
| on the left-hand side | on the right-hand side
--- | --- | ---
top | A | B
bottom | B | A

Fitting assembly for equipping a door :

- (1) fixed hinge
- (2) moving hinge
- (3) bolt
- (4) shaft
- (5) centralising pin

The shim [2] at (C) (13 mm dimension to the outside) .

The shim [3] at (D) (15 mm dimension to the outside) .

The 2 thrust shims [4] 13 mm thick at (E) .

Fit the hinges (1) on the centre pillar .

Half-tighten the bolts (3) .

Position the door opposite the hinges .

Tighten, without locking, the hinge bolts (2) to the door .

Tighten the check strap on the centre pillar .

NOTE : the door hinge pin holding bolts (4) face each other .

Close the door and check the clearances :

- height (E) : 5 ± 2 mm
- clearances (F) : 4 ± 1.5 mm
- flush fitting : 0 mm

Open the front door .

Keep the rear door closed .

Tighten the bolts (3) .

Secure the check strap on to the centre pillar .

Check the fits and clearances .

NOTE : in the event of difficulty in closing .

Remove :

- remove the centralising pin (5) on the door hinge
- if necessary enlarge the diameter of the drilled housings (6) of the guides (7)
- if this is not sufficient, grind the guides (7)

For these operations, repeat the surface treatment (Application of an anti-corrosion product) .

Check the fits and clearances .

NOTE : in the event of difficulty in adjustment between the striker and the locks, fit a 306 type striker without indexing to be able to make the adjustment .

Tighten the fastenings :

- (2) 2 da.Nm
- (4) 1.4 da.Nm