B3DB03V1 - 206

DATA - TIGHTENING TORQUE(S) REAR SUSPENSION

1 - DATA

1 - 1 - SUSPENSION

engine code | HFY HFZ | HFY HFZ | HFY HFZ
--- | --- | --- | ---
special features | tyres 165/70 R 13 | tyres 175/65 R 14 | 'Affaire'
anti-roll bar diameter (mm) | N/A | N/A | 18
diameter of torsion bar (mm) or spring (colour reference) | 19.5 | 19.5 | 19.5
length of the adjusting tool (mm) | 370 | 367 | 371

engine code | HFY HFZ | KFX K6C | KFX K6C
--- | --- | --- | ---
special features | overseas export | tyres 165/70 R 13 | tyres 175/65 R 14
anti-roll bar diameter (mm) | 19 | 18 | 18
diameter of torsion bar (mm) or spring (colour reference) | 19.5 | 19 | 19
length of the adjusting tool (mm) | 385 | 377 | 375

engine code | KFX K6C | NFZ HFZ | NFZ | RFR | WJZ WJY
--- | --- | --- | --- | --- | ---
special features | overseas export | without | overseas export | without | without
anti-roll bar diameter (mm) | 19 | 20 | 19 | 22 | 19
diameter of torsion bar (mm) or spring (colour reference) | 19.5 | 19 | 19.5 | 19.5 | 19
length of the adjusting tool (mm) | 385 | 375 | 385 | 367 | 374

engine code | WJZ WJY | WJZ WJY | RHY | RHY
--- | --- | --- | --- | ---
special features | 'Affaire' | overseas export | without | overseas export
anti-roll bar diameter (mm) | 18 | 19 | 21 | 19
diameter of torsion bar (mm) or spring (colour reference) | 19.5 | 19.5 | 19 | 19.5
length of the adjusting tool (mm) | 371 | 385 | 375 | 385

1 - 2 - REAR SUSPENSION GEOMETRY

engine code | HFY HFZ | HFY HFZ | HFY HFZ
--- | --- | --- | ---
special features | tyres 165/70 R 13 | tyres 175/65 R 14 | 'Affaire'
H2 (mm) | 118 | 121 | 98
camber | -1° ± 30' | -1° ± 30' | -1° ± 30'
track - wheel (mm) | + 1.5 ± 0.5 | + 1.7 ± 0.5 | + 2.1 ± 0.5
track - wheel (°) | + 0° 16' ± 5' | + 0° 16' ± 5' | + 0° 22' ± 5'
track : + toe-in - toe-out these values are for a reference height (H2)

engine code | HFY HFZ | KFX K6C | KFX K6C
--- | --- | --- | ---
special features | overseas export | tyres 165/70 R 13 | tyres 175/65 R 13
H2 (mm) | 149 | 121 | 121
camber | -1° ± 30' | -1° ± 30' | -1° ± 30'
track - wheel (mm) | + 1 ± 0.5 | + 1.5 ± 0.5 | + 1.7 ± 0.5
track - wheel (°) | + 0° 10' ± 5' | + 0° 16' ± 5' | + 0° 16' ± 5'
track : + toe-in - toe-out these values are for a reference height (H2)

engine code | KFX K6C | KFX K6C | NFZ
--- | --- | --- | ---
special features | 'Affaire' | overseas export | without
H2 (mm) | 109 | 149 | 121
camber | -1° ± 30' | -1°±30' | -1°±30'
track - wheel (mm) | +2.1±0.5 | +1±0.5 | +1.7±0.5
track - wheel (°) | +0°22'±5' | +0°10'±5' | + 0°16'± 5'
track : + toe-in - toe-out these values are for a reference height (H2)

engine code | NFZ | RFR | RFR
--- | --- | --- | ---
special features | overseas export | without | Grand Tourisme
H2 (mm) | 149 | 121 | 128
camber | -1°±30' | -1°±30' | -1°±30'
track - wheel (mm) | +1±0.5 | +1.7±0.5 | +1.7±0.5
track - wheel (°) | +0°10'±5' | +0°16'± 5' | +0°16'±5'
track : + toe-in - toe-out these values are for a reference height (H2)

engine code | WJZ WJY | WJZ WJY | WJZ WJY
--- | --- | --- | ---
special features | without | 'Affaire' | overseas export
H2 (mm) | 121 | 109 | 149
camber | -1° ± 30' | -1° ± 30' | -1° ± 30'
track - wheel (mm) | + 1.7 ± 0.5 | + 2.1 ± 0.5 | + 1 ± 0.5
track - wheel (°) | + 0° 16' ± 5' | + 0° 22' ± 5' | + 0° 10' ± 5'
track : + toe-in - toe-out these values are for a reference height (H2)

engine code | RHY | RHY | RHY
--- | --- | --- | ---
special features | without | 'Affaire' | overseas export
H2 (mm) | 121 | 123 | 149
camber | -1° ± 30' | -1° ± 30' | -1° ± 30'
track - wheel (mm) | + 1.7 ± 0.5 | + 2.1 ± 0.5 | + 1 ± 0.5
track - wheel (°) | + 0° 16' ± 5' | + 0° 22' ± 5' | + 0° 10' ± 5'
track : + toe-in - toe-out these values are for a reference height (H2)

(H2) Height from ground to rear jacking point, at reference height .

2 - TIGHTENING TORQUE(S)

reference / description | da.Nm
--- | ---
special features | without
(1) flexible mount to body fastening | 11
(2) flexible mount to body fastening | 11
(3) torsion bar | 1.9
(4) rear shock absorber fastening to yoke | 7
(5) rear shock absorber fastening to arm | 15
(6) rear hub fastener | 20
(7) anti-roll bar lever bolt | 3.6