B2CK00K1 - 206 MA GEARBOX

CLEANING AND REFITTING CONDITIONS GEARBOX

Do not use abrasives or sharp tools on the joint faces .

Clean the threads in the cylinder block with a tap .

Fit only parts which are clean and free from faults (scores, burrs, knocks...) .

Oil the parts one by one as they are refitted .

Always renew after removal :

- the seals
- the pins
- the bearings
- the bearing guide
- spring rings and circlips
- the spring washers
- the bearing guide tube tightening bolts
- the clutch shaft bearings
- the shaft line tightening nuts
- the intermediate plate tightening bolts
- the differential pinion shaft circlip

Maintain the matching of :

- the clutch housing and the intermediate plate
- the selection lever and shaft
- of the clutch release shaft and lever
- the engagement finger and lever
- the forks and shafts

Preliminary operations :

- operations which must be carried out before beginning the method

Complementary operation(s) :

- operations which must be carried out after completing the method in order to make the gearbox operational again