C5DH05F1 - 206

REPLACEMENT DOOR LOCK

1 - TOOLING

[1] Lock removal tool .

2 - REMOVAL

Remove the blank from the door shut face .

Screw the tool fully into the fork .

Pull the assembly to release the fork from the lock .

Remove the lock by pivoting it .

3 - REFITTING

Fit the lock closely against the door .

Gently engage the fork .

Push the fork fully into the lock .

Check that the lock is securely held before removing the tools .

Proceed in the reverse order to removal .