C5FG1KF1 - 206

REMOVAL - REFITTING FASCIA

1 - REMOVAL

Disconnect the battery .

Remove :

- the steering wheel module (1) (refer to the procedure check - repairs - adjustment air bags)
- the steering wheel (2) marking its position on the splines
- the central console (3)
- the lower trim (4) under the steering wheel
- the side switches (5) (according to specification)
- the blanks (6)
- the steering column

Pull the lower section of the visor (7) to detach it .

Finish unclipping the upper section .

Remove the binnacle (7) .

Remove the fastener (8) .

Disconnect the instrument panel connectors .

Remove the instrument panel (9) .

Unclip the upper centre panel (10) by pulling it towards you .

Disconnect the hazard warning lights switch (11) .

Remove the fasteners (12) .

Disconnect the connector .

Remove the clock (13) or the display (According to specification) .

Remove the panel (14) or the radio (According to specification) .

Remove the fasteners (15) .

Unclip the centre panel (16), by pulling it gently towards you .

Remove the centre panel (16) .

Remove the fasteners (17) - (18) - (19) .

Remove the fastener (20) .

Remove the fastener (21) for the earth lead .

Remove the fasteners (22) .

Disconnect the connector (23) .

Remove the fastener (24) .

For the following operations, two operators are necessary : On each side, lift the fascia and pull it towards you to detach it from the air conditioner and the windscreen .

Remove the fascia .

2 - REFITTING

Proceed in the reverse order to removal .

3 - TIGHTENING TORQUE(S)

WARNING : follow the tightening sequence (the torques for the mountings which secure the fascia to the body after clipping) .

Fastener (20) : 1,9 da.Nm .

Fastener (22) : 1,9 da.Nm .

Fastener (24) : 1,9 da.Nm .