C4AG0JF1 - 206

REMOVAL - REFITTING FRONT WING

1 - REMOVAL

Open the bonnet .

Remove :

- the grille (upper part)
- the grille (lower part)
- headlight

Remove :

- the fasteners (1)
- the clip (2)
- the mud shields

Disconnect the wing repeater .

Open the door .

Slacken the mounting (3) passing via the interior of the wing .

Remove the fasteners (4) .

NOTE : on the left-hand side : secure the bonnet .

Remove :

- bonnet stay

Remove the fasteners (5) .

Release the wing by removing it from its mountings .

Press on the bumper .

Remove the front wing .

2 - REFITTING

NOTE : on the left-hand side : apply a 2 x 8 x 400 mm bodywork mastic filler and sealer between the wing inner panel and the wing flange .

Insert the wing in the centralising stop (A) .

Proceed in the reverse order to removal .

Adjust the flush fitting at the upper section .

Check the operation of the electrical equipment .