B2CI06K1 - 206 MA GEARBOX

DRAINING - FILLING - LEVEL GEARBOX

1 - SPECIAL TOOLS

[1] Drain plug spanner (-).1402 .

[2] Type manual oil syringe FACOM 376 .

[3] Pneumatic gearbox filler RH 100 .

2 - DRAINING - FILLING - LEVEL GEARBOX

NOTE : in the case of frequent contact of the skin with the lubricant, it is recommended that protective gloves are worn .

Drain plug (1); Tightening torque : 2.5 da.Nm .

Filler and level plug (2); Tightening torque : 2.5 da.Nm .

Drain the gearbox when warm .

Always replace the drain and top-up plug seal .

Shake the new can of oil before use to make the mixture uniform (the additives settle at the bottom of the can) .

Oil capacity : 2 litre(s) .

Recommended fluid :

- ESSO GEAR OIL BV 75W-80W
- TOTAL TRANSMISSION BV 75W-80W ;new formula