C5KG0DF1 - 206

REMOVAL - REFITTING ELECTRIC SUNROOF

1 - REMOVAL

Remove :

- the headlining
- the interior tailgate frame

Remove the fastenings .

Two people are required to perform the following operation .

Remove the sun roof .

2 - REFITTING

Check the condition of the seals on the sun roof frame .

Check that the cable guides are in place .

Clean the roof before refitting the sun roof .

Proceed in the reverse order to removal .

Tightening order : (1) to (9) :

- tighten the fasteners to 0,25 da.Nm