C5IG19F1 - 206 CABRIOLET

REMOVAL - REFITTING REAR SCREEN LOWER SEAL

1 - REMOVAL

APPLY THE HYDRAULIC PUMP LOAD REDUCTION OPERATION .

IMMOBILISE THE BOOT COVER .

Loosen the seal (1) completely .

2 - REFITTING

NOTE : apply a product to assist fitting on the flange (example: soapy water) .

Position the ends of the seal (1) fully against the lower moulding of the upper seal of the rear screen (2) fitting the clip correctly on the rubber covering (at A) .

Fit the seal (1) taking care not to turn the clip base lip (3) over on itself .

Take the bead (4) in the centre and pull it towards each of the two ends (fit the lip thus on the panel) .

WARNING : fit the bead (4) correctly at the two grooves R1 - R2 .

Proceed in the reverse order to removal .

Carry out :

- an operation test
- A BOOT SEALING TEST