C4DH0IF1 - 206 CABRIOLET

REPLACEMENT CROSSMEMBER STIFFENER WINDSCREEN APERTURE UPPER CROSSMEMBER INNER PANEL

IMPERATIVE : THIS VEHICLE HAS BEEN DESIGNED USING THE MIG BRAZE WELDING TECHNIQUE ; when the structure is repaired, all the connections concerned must be welded using the same procedure ; any other technique is prohibited .

WARNING : all the scoured areas must be protected by the approved electrolytic re-zincing process .

IMPERATIVE : observe elementary health and safety rules (wearing of filter mask for organic fumes - work in a ventilated area) .

1 - COMPLEMENTARY OPERATION(S)

Replacement :

- windscreen aperture upper crossmember

2 - IDENTIFICATION OF REPLACEMENT PARTS

(1) Windscreen aperture upper crossmember stiffener .

(2) Windscreen aperture upper crossmember inner panel .

3 - PART(S) REQUIRED TO CARRY OUT THE OPERATION

(1) Windscreen aperture upper crossmember stiffener .

(2) Windscreen aperture upper crossmember inner panel .

4 - CUTTING OUT

5 - RELEASING

6 - WELDING