C4CG20F1 - 206 CABRIOLET

REMOVAL - REFITTING DOOR ASSEMBLY

1 - TOOLING

[1] Door stand CELETTE .

2 - REMOVAL

Lower the window .

Place the stand [1] under the door .

Remove the door check strap (1) .

Disconnect the connector (2) .

Remove the pins (3) from the hinges .

Detach the door and its support .

3 - REFITTING

Proceed in the reverse order to removal .

Tighten the fastener (1) to 2.2 daN.m. .

Carry out an electrical operation check .