B2FH02K1 - 206

REPLACEMENT DRIVE SHAFT BEARING ALL TYPES

1 - SPECIAL TOOLS

reference | description | reference | reference
--- | --- | --- | ---
[1] | drive shaft bracket | (-).0403-R | (-).0403-R

reference | description | reference | reference
--- | --- | --- | ---
[2] | drive shaft retaining ring ø 72 mm | (-).0410-D | 4101-T

reference | description | reference | reference
--- | --- | --- | ---
[3] | drive shaft retaining ring ø 65 mm | (-).0410-F | 4518-T

reference | description | reference | reference
--- | --- | --- | ---
[4] | spider protector | (-).0410-J1 (-).0410-J2 (-).0410-J3 (-).0410-J4 | (-).0410-J1 (-).0410-J2 (-).0410-J3 (-).0410-J4

reference | description | reference | reference
--- | --- | --- | ---
[5a] | tool for fitting the MB3 automatic gearbox adapter sleeve | (-).0410-G | 4608-TH
[5b] | tool for fitting the AL4 automatic gearbox adapter sleeve | (-).0410-K | (-).0410-K

reference | description | reference | reference
--- | --- | --- | ---
[6] | tool for fitting the bearing | (-).0410-BZ | 0410-BZ

reference | description | reference | reference
--- | --- | --- | ---
[7] | mechanical bolt cross-piece | FACOM U 53 K2 | FACOM U 53 K2
[8] | stripping device | FACOM U 53 T2 | FACOM U 53 T2

reference | description | reference | reference
--- | --- | --- | ---
[9] | replacement tie-rod | FACOM U 53 RL | FACOM U 53 RL
[10] | adaptor | FACOM U 53 H | FACOM U 53 H

[11] Clips-bindings fitting kit .

reference | description | reference | reference
--- | --- | --- | ---
[12] | tripod fitting drift | (-).0410-C | 4101-T

reference | description | reference | reference
--- | --- | --- | ---
[13] | CLIC clip pliers | (-).0409 | 4178-T

reference | description | reference | reference
--- | --- | --- | ---
[14] | clip pliers : OETIKER | (-).0408 | 4151-T

2 - REPLACEMENT OF THE BEARING

Uncouple the joint at the gearbox end (A) .

Using a press and the tool [8], remove the stop ring (2) and the bearing (3) simultaneously .

Other procedure :

- using the tools [8], [7] and [9], remove the stop ring (2) and then the bearing (3)

Refit a new bearing and stop ring simultaneously using the tool [6] .

Fit a new O-ring .

Clean and grease the splines .

Special feature : Automatic gearbox .

Extract the sleeve (1) using the tools [12] and [8] .

Refit the sleeve using the tool [5a] or [5b] :

- reference G : for MB3 automatic gearbox
- reference K : for autoadaptive gearbox