C4CG28F1 - 206 CABRIOLET

REMOVAL - REFITTING : EXTERIOR DOOR WEATHERSTRIP

1 - REMOVAL

Lower the window .

UNSCREW THE MIRROR MOUNTINGS .

Remove :

- the clips (1)
- the exterior weatherstrip (2)

2 - REFITTING

NOTE : apply a product to assist fitting on the flange (example: soapy water) .

Fit the weatherstrip (2) at the front .

Push the weatherstrip forwards to position it in relation to the door panel, at the rear .

Finish fitting the seal .

Tighten the mirror mountings .

Raise the glass .