C5AH00K1 - 206

REPLACEMENT BONNET OPENING CABLE

1 - RECOMMENDED TOOLS

Contents of kit (Workshop reference (-).1324) .

[1] Shim .

[2] Sleeve (wire feed) .

[3] Pliers .

[4] Gripping tool .

2 - REMOVAL

Operate the bonnet opening control .

Remove :

- the bottom trim (1)
- the fastener (2)

Release the opening control (3) .

Remove :

- the Built-in Systems Interface

Unclip the radiator grille upper protective grille .

Unclip :

- the cable (4) on the lock (5)

Tape the sleeve [2] onto the cable (4) .

Pull the cable from the passenger compartment .

3 - REFITTING

Attach the sleeve [2] to the new cable .

Coat the sleeve with soapy water .

Pull on the sleeve [2] .

Guide the cable along the wing .

Remove the sleeve [2] .

Pull on the grommet using the pliers [3] .

Hook the cable (4) onto the lock (5) .

Proceed in the reverse order to removal .

Tighten :

- the bolt (2) to 0,6 da.Nm