C4CG29F1 - 206 CABRIOLET

REMOVAL - REFITTING : DOOR WEATHERSTRIP END PIECE

1 - REMOVAL

Lower the window .

REMOVE THE DOOR TRIM PAD .

Remove the clips (1) .

Using a 10 mm dia. drill bit, drill rivets (2) .

Retrieve the rivets which have fallen in the base of the door .

Remove :

- the bracket (3)
- the end piece (4) upwards

2 - REFITTING

Position the weatherstrip end piece on the flange .

Position the support (3) and fit the new rivets (2) .

Press on the weatherstrip end piece following (A) to clip it in this area .

Fit new clips (1) .

Continue the fitting operations in the reverse order to removal .