C4AG0RF1 - 206 CABRIOLET

REMOVAL/REFITTING OF WINDSCREEN APERTURE UPPER TRIM

1 - REMOVAL

Using a spatula [1], unclip the lamp (1) .

Disconnect the harness (2) from the ceiling light .

Press the retaining lugs (3) of the console .

Tilt, then remove the roof console (4) .

Remove :

- the fasteners (5)
- the fastener (6)
- the sun visor
- the sun visor retaining hooks

Gradually unclip then remove the windscreen aperture upper trim (7) .

2 - REFITTING

Proceed in the reverse order to removal .