C4DG09F1 - 206

REMOVAL - REFITTING ELECTRIC SUN ROOF INTERIOR PANEL FRAME

1 - REMOVAL

Remove the headlining .

Remove the fasteners : (1) to (16) .

Two people are required to perform the following operation .

Remove the sun roof frame and remove it via the rear of the vehicle .

2 - REFITTING

Proceed in the reverse order to removal .

Follow the tightening sequence : (1) to (16) .

Tighten the fasteners to 0,2 da.Nm .