C4BH31F1 - 206 CABRIOLET

REPLACEMENT REAR WING ASSEMBLY

IMPERATIVE : this vehicle has been designed using the mig brazing process technique ; when the structure is repaired, all the connections concerned must be welded using the same procedure ; any other technique is prohibited .

WARNING : all the scoured areas must be protected by the approved electrolytic re-zincing process .

IMPERATIVE : observe elementary health and safety rules (wearing of filter mask for organic fumes - work in a ventilated area) .

1 - SPECIAL FEATURE

On adjustment of the rear wing assembly, use either the jig tools or mechanical or electronic measuring equipment .

2 - COMPLEMENTARY OPERATION(S)

Removal - refitting :

- REAR BUMPER
- tail lamp
- QUARTER LIGHT - REAR QUARTER PANEL WINDOW MECHANISM
- DOOR STRIKER
- door aperture seal
- TAILGATE APERTURE SEAL
- REAR QUARTER PANEL INTERIOR WEATHERSTRIP SEAL
- REAR QUARTER PANEL EXTERIOR WEATHERSTRIP
- FUEL TANK (right-hand side)
- REAR QUARTER PANEL WEATHERSTRIP END PIECE
- rear mud shield
- wing protector side moulding
- front seat belt inertia reel

Remove-refit trim :

- rear wing inner panel

Detach the electrical harnesses .

Protect :

- the fuel pipes (right side)
- the front carpet and boot carpet

3 - IDENTIFICATION OF REPLACEMENT PARTS

Rear wing assembly .

4 - REPLACEMENT PART COMPOSITION

(1) : Rear wing .

(2) : Rear wing stiffener .

(3) : Rear light housing upper closer .

(4) : Rear light outer housing .

(5) : Rear light inner housing .

(6) : Passenger compartment bottom rear closer .

5 - PART(S) REQUIRED TO CARRY OUT THE OPERATION

Rear wing assembly .

6 - PREPARATION OF THE NEW PART

7 - CUTTING OUT

8 - RELEASING

9 - ADJUSTMENT

10 - WELDING

11 - SEALING

12 - PROTECTION