C5IM01F1 - 206 CABRIOLET

CLOSING THE ROOF (MANUAL REPAIR PROCEDURE FROM CABRIOLET TO COUPÉ)

Lower the 4 side windows .

Open the luggage compartment .

Fold up the tray (luggage cover screen) (1) .

CARRY OUT THE HYDRAULIC UNIT LOAD REDUCTION OPERATION AT (A) .

Pull the cord (2) to fold the moving rear shelf .

IMMOBILISE THE BOOT COVER .

Lift the roof, then unfold it gradually towards the front .

Place the roof in contact with the front section of the windscreen aperture, then lock the roof onto the strikers .

Remove the sided spanner from the guide .

Fold down the boot cover to the front by lightly pressing in the centre of the cover to counter the residual pressure of the system .

Open the luggage compartment .

On each side :

- A : pull the u-clip (3)
- B : pivot the u-clip (3) and release it

Check that the boot cover is locked .

Close the boot .

Raise the door side windows and the quarter lights .

Following elimination of the fault, do not forget to return the u-clip (3) to its initial position .