C5CG0ZF1 - 206

REMOVAL - REFITTING ELECTRIC CONCEALING BLIND MOTOR

1 - REMOVAL

Open the concealing blind .

Remove :

- the sun visors
- the sun visor retaining hooks
- the roof console
- the front grab handles
- the screen blind frame finisher seal
- partly : the screen pillar trim pads

Release the headlining from the front door seals .

WARNING : lower the headlining at the front taking care not to fold it .

Disconnect the electrical connection (1) .

Unclip the roof console bracket (2) .

Remove the mountings from the engine (3) .

Uncouple the motor from the mechanism .

Remove the motor (4) .

2 - REFITTING

IMPERATIVE : check : the coupling of the motor to its mechanism .

Proceed in the reverse order to removal .