C5CG0XF1 - 206

REMOVAL - REFITTING SHUTTERS OF THE CONCEALING BLIND

IMPERATIVE : store the concealing blind in its housing .

Remove the headlining .

Remove the concealing blind sub-assembly .

NOTE : to carry out the following operation, place the concealing blind sub-assembly on a clean support .

1 - REMOVAL

Re-close the concealing blind using its motor and leave it approx. 40 mm open .

WARNING : removal of the flaps of the concealing blind is from the front towards the rear of the vehicle .

Seat the flap (1) on a side guide (2), bend it in the middle and release it from its guides .

2 - REFITTING

WARNING : refitting the flaps of the concealing blind is from the rear towards the front; observe the direction of assembly (rounded section to the rear) .

Continue refitting the following flaps .

Check operation .

Continue the fitting operations in the reverse order to removal .