B2CB4EK1 - 206 BE4 GEARBOX

IDENTIFICATION, DATA, TIGHTENING TORQUE(S) MANUAL GEARBOX

1 - IDENTIFICATION

Identification area (A) comprising :

- the component reference
- serial number

2 - DATA

engine code | WJZ - WJY | WJZ - WJY | WJZ - WJY
--- | --- | --- | ---
special features | 175/70R13 tyres | 175/65R14 tyres | 175/70R13 tyres
unit reference | 20DL12 - 20DL13 - 20DL22 - 20DL23 | 20DL12 - 20DL13 - 20DL22 - 20DL23 | 20DL02 - 20DL03 - 20DL24 - 20DL25
gearbox type | BE4/5 | BE4/5 | BE4/5
gearbox ratios ; 1st | 11 x 38 | 11 x 38 | 11 x 38
gearbox ratios ; 2nd | 23 x 43 | 23 x 43 | 23 x 43
gearbox ratios ; 3rd | 25 x 32 | 25 x 32 | 25 x 32
gearbox ratios ; 4th | 41 x 39 | 41 x 39 | 41 x 39
gearbox ratios ; 5th | 47 x 35 | 47 x 35 | 47 x 35
gearbox ratios ; reverse | 12 x 31 x 40 | 12 x 31 x 40 | 12 x 31 x 40
speed at 1000 revs/min (in km/h) ; 1st | 8.55 | 8.61 | 8.10
speed at 1000 revs/min (in km/h) ; 2nd | 15.80 | 15.90 | 14.96
speed at 1000 revs/min (in km/h) ; 3rd | 23.08 | 23.23 | 21.86
speed at 1000 revs/min (in km/h) ; 4th | 31.06 | 31.26 | 29.41
speed at 1000 revs/min (in km/h) ; 5th | 39.68 | 39.92 | 37.57
speed at 1000 revs/min (in km/h) ; reverse | 8.86 | 8.91 | 8.38
final drive ratio(s) | 17 x 61 | 17 x 61 | 19 x 72
speedometer drive | 19 x 17 | 19 x 17 | 19 x 17
differential diameter | UNK. | UNK. | UNK.
oil capacity ; litre(s) | 1.9 | 1.9 | 1.9

engine code | WJZ - WJY | WJZ - WJY | WJZ - WJY
--- | --- | --- | ---
special features | 175/65R14 tyres | 185/55R15 tyres | 175/65R14 tyres
unit reference | 20DL02 - 20DL03 - 20DL24 - 20DL25 | 20DL08 - 20DL09 | 20DL06 - 20DL07
gearbox type | BE4/5 | BE4/5 | BE4/5
gearbox ratios ; 1st | 11 x 38 | 11 x 38 | 11 x 38
gearbox ratios ; 2nd | 23 x 43 | 23 x 43 | 23 x 43
gearbox ratios ; 3rd | 25 x 32 | 25 x 34 | 27 x 31
gearbox ratios ; 4th | 41 x 39 | 39 x 41 | 45 x 37
gearbox ratios ; 5th | 47 x 35 | 43 x 37 | 47 x 31
gearbox ratios ; reverse | 12 x 31 x 40 | 12 x 31 x 40 | 12 x 31 x 40
speed at 1000 revs/min (in km/h) ; 1st | 8.15 | 8.16 | 8.38
speed at 1000 revs/min (in km/h) ; 2nd | 15.06 | 15.08 | 15.49
speed at 1000 revs/min (in km/h) ; 3rd | 21.99 | 23.73 | 25.22
speed at 1000 revs/min (in km/h) ; 4th | 29.60 | 26.82 | 35.22
speed at 1000 revs/min (in km/h) ; 5th | 37.80 | 32.77 | 43.90
speed at 1000 revs/min (in km/h) ; reverse | 8.45 | 8.45 | 8.69
final drive ratio(s) | 19 x 72 | 19 x 72 | 19 x 70
speedometer drive | 19 x 17 | 22 x 18 | 19 x 17
differential diameter | UNK. | UNK. | UNK.
oil capacity ; litre(s) | 1.9 | 1.9 | 1.9

3 - TIGHTENING TORQUE(S)

engine code | da.Nm
--- | ---
special features | without
(2) gearbox rear casing | 1.25
(3) securing the gearbox casing to the clutch housing | 1.25
(4) reverse gear rocking shaft securing nut | 4.5
(5) breather | 1.5
(6) reverse lamp switch | 2.5
(7) drain plug | 3.5
(8) level plug | 2.2
(9) speedometer drive support | 1.5
(10) differential housing fastener | 1.25
(11) differential housing fastener | 5
(12) thrust bearing guide fastening | 1.25
(13) differential extension fastener | 1.5
(14) stop plate fastener | N/A
(15) gearbox mounting on crankcase | 5.5

engine code | da.Nm
--- | ---
special features | without
(20) input shaft nut | 7.25
(21) output shaft nut | 6.5
(22) bearing retaining bolt | 1.5
(23) gearbox control bracket bolts | 1.5
(24) differential crown wheel fastener | 6
(25) fork securing bolts | N/A