B3EK01K1 - 206

GENERAL PRECAUTIONS POWER STEERING WITH INTEGRAL RAM

You are going to carry out work on power steering with integral ram .

The reliability of the mechanism depends on the quality of your work .

Consequences of impurities in the system :

- seizure of the mechanism
- jamming of the mechanism
- fluid leaks
- power steering loss

General precautions :

- use new fluid when filling and topping up the system
- use plugs (available from Parts Division) to close the openings of the valve and the pipes
- follow the instructions of the various repair procedures
- carry out the work in a very clean area
- use lint-free cloths
- do not use an air nozzle